|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name of activity, event, and location** | **Powerboats** | **Date of risk assessment** | **Feb 2025** | **Name of person doing this risk assessment** | **David Morton****Review:****Ray Hardman** |
| **Date of next review** | **Feb 2026** |

|  |  |  |  |
| --- | --- | --- | --- |
| **What hazard have you identified?****What are the risks from it?** | **Who is at risk?** | **How are the risks already controlled?****What extra controls are needed?** | **What has changed that needs to be thought about and controlled?** |
| **Powerboat Launch & Recovery** | **Crew,****Launch crew** | **Operators should be suitably trained in the use of vehicle/trailer and the launching/recovery procedure for each boat.****Operator must be aware of the Use of Vehicles SOP/RA****Ensure persons not taking part in the launch are clear of the slipway.** |  |
| **Fuel Spillage** | **Crew** | **Refuelling must take place off the boat.** **Fuel Tanks must be kept secure in the fuel bunker when not in use.****Spillages must be cleaned up (spill kit provided in fuel bunker)** |       |
| **Man Overboard**  | **Crew,****Rescued Persons** | **All safety boat crew are qualified to RYA standards as per the SOP****Helm to drive at a safe speed at all times.****Kill cord must be worn at all times when engine is running.****The driver should test the kill cord for correct operation at the beginning of every session** |  |
| **Fire** | **Crew & Participants** | **Fuel tank must be secured at all times.****Integrity of fuel lines must be checked to ensure no leakage of fuel into the boat.****No smoking on board.****In the event of a fire on board, use the extinguisher if safe to do so or abandon the boat.** |  |
| **Swamping** | **Crew & Participants** | **Boats should not be overloaded.****Boat should only be on the water in suitable conditions.** |  |
| **Collision** | **Crew & Participants** | **Helm should be aware of the IRPCS.****Care should be taken when approaching other craft.** |  |
| **Mechanical Failure** | **Participants** | **In the event of a failure the anchor should be deployed.****If necessary, the activity should be halted until adequate Safety cover is available with other powerboats.** |  |
| **Propeller Injury** | **Crew & Participants** | **Engine should be stopped when the boat is in the vicinity of persons in the water.** |  |